**Supply of Edge Switch (1):**

|  |  |  |
| --- | --- | --- |
| **Sl.no** | **Attribute** | **Specification** |
| 1 | Type | 8 port L2 or above Manage switch with cisco equivalent |
| 2 | Ports | 8-ports 10/100/1000 + 2 combo Gigabit SFP |
| 3 | POE | POE and POE+ |
| 4 | Warranty | 1 year product warranty |
| Unit:-NoRate………………………………….. |

|  |  |  |
| --- | --- | --- |
| **Sl.no** | **Attribute** | **Specification** |
| 1 | Type | 24 port L2 or above Manage switch with cisco equivalent |
| 2 | Ports | 24-ports 10/100/1000 + 4 combo Gigabit SFP |
| 3 | POE | POE and POE+ |
| 4 | Warranty | Minimum 1 year product warranty |
| Unit:- NoRate:- ………………………………. |

|  |  |  |
| --- | --- | --- |
| **Sl.no** | **Attribute** | **Specification** |
| 1 | Type | 48 port L2 or above Manage switch with cisco equivalent |
| 2 | Ports | 48-ports 10/100/1000 + 4 combo Gigabit SFP |
| 3 | POE | POE and POE+ |
| 4 | Warranty | Minimum 1 year product warranty |
| Unit:- NoRate………………………………………….. |